60311AV - Support rail - 32 mm diameter - With virucidal film
300 mm straight bar. Presto type ref. 60311AV or technically equivalent.  Brushed stainless steel finish, diameter 32 mm. With transparent COVERSAFE ™ virucidal film, and destruction of 99.9% of viruses and bacteria in 24 hours. Efficiency tested and validated for 4 years.Delivered with rosettes of finish to clip