60378 - Wall-mounted compact automatic touch free hand dryer, matte black
Wall-mounted compact automatic touch free hand dryer Presto C-DRY (réf. 60378) or technically equivalent. Operated automatically by hand detection. Wall-mounted. Mains-operated: 220V-240VAC. Smart temperature regulator with 3 security levels. Anti-blocking system after 60 seconds. Power 1000W. Fast dry 10 to 15sec. Air speed: 95 à 115 m/s (342 à 414 km/h). Drip Proof IP24. Electrical class: 1.  Matte black finish. 

60378 - Wall-mounted compact automatic touch free hand dryer, matte black
Wall-mounted compact automatic touch free hand dryer Presto C-DRY (réf. 60378) or technically equivalent. 
- Operated automatically by hand detection. 
- Wall-mounted. 
- Mains-operated: 220V-240VAC. 
- Smart temperature regulator with 3 security levels. 
- Anti-blocking system after 60 seconds. 
- Power 1000W. Fast dry 10 to 15sec. 
- Air speed: 95 à 115 m/s (342 à 414 km/h). 
- Drip Proof IP24. 
- Electrical class: 1.  
- Matte black finish.