64677 - Wall-mounted sensor and timed-flow single tap - 1.9l/min
Sensor wall-mounted tap Presto SAFE® ref 64677 or technically equivalent. With detection cell and solenoid valve integrated. 9V Lithium battery delivered with the tap. G 1/2" connection, 7 sec adjustable flow time, integrated spray flow regulator (1,9l/min), 30 sec adjustable automatic rinsing every 24h after last use, chrome finish. 

64677 - Wall-mounted sensor and timed-flow single tap - 1.9l/min
Sensor wall-mounted tap Presto SAFE® ref 64677 or technically equivalent. Including :
- Detection cell
- Delivered 9V lithium battery
- Integrated solenoid valve. 
- G 1/2" connection, 
- 7 sec adjustable flow time, 
- Integrated spray flow regulator (1,9l/min), 
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish