64679 - Deck-mounted sensor and timed-flow single tap - 3l/min
Single deck-mounted sensor tap Presto SAFE® ref 64679 or technically equivalent. With detection cell and solenoid valve integrated. 9V Lithium battery delivered with the tap. G 1/2" connection, 7 sec adjustable flow time, integrated flow regulator (3l/min), 30 sec adjustable automatic rinsing every 24h after last use, chrome finish. 

64679 - Deck-mounted sensor and timed-flow single tap - 3l/min
Single deck-mounted sensor tap Presto SAFE® ref 64679 or technically equivalent. Including :
- Detection cell
- Delivered 9V lithium battery
- Integrated solenoid valve. 
- G 1/2" connection, 
- 7 sec adjustable flow time, 
- Integrated flow regulator (3l/min), 
- 30 sec adjustable automatic rinsing every 24h after last use
- Chrome finish