70808 - Deck-mounted mixer tap with 2 holes – upward spout
Two-hole deck mixer with upward spout. Swivel spout, projection 308 mm, height under spout 296 mm, diameter 22 mm. 1/4 turn ceramic head with flow rate of 81L/min at 3 bar. Interchangeable anti-limescale star-shaped flow straightener. Chromed brass body and spout. Reference 70808, brand PRESTO or equivalent.

70808 - Deck-mounted mixer tap with 2 holes – upward spout
Two-hole deck-mounted mixer with upward spout, Reference 70808, brand PRESTO or equivalent, including:
- Swivel spout, projection 308 mm, height under spout 296 mm, diameter 22 mm
- 1/4 turn ceramic head with flow rate of 81L / min at 3 bar
- Interchangeable anti-limescale star-shaped flow straightener
- Chromed brass body and spout