75030 - 
Sink mixer, 150mm span, no drain, 150 mm tube spout, wall-mount with solid handle. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow and flow settings from 2l to 13.8l/min. Body and control in polished chrome plated brass. Star shaped flow straightener, M24 x 1. Connection LN G'3 / 4 comes with rosettes and off-centre fittings M G’1/2 10 year warranty. Sanifirst brand shower mixer, 150mm span REF: 75030 or approved equivalent.