75391 - Sink mixer with swivel spout
Single hole sink mixer without drain for handwash basin, deck-mount with solid handle. Extruded spout, swivel, removable L 235mm. Height to nozzle 135mm. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow and flow settings from 2l to 12l/min. Tapware fitted as standard with aerator M 24x1. Smooth body, spout and controls in polished chrome plated brass. EPDM Hoses, M12x1, LN G'3 / 8 L 350mm Reinforced fixation by a stainless steel rod. 10 year warranty. Sanifirst brand Single hole sink mixer, swivel, extruded spout REF: 75391 or approved equivalent.