85755 - SAFETY SHOWER FOR EXPOSED PIPEWORK 
Safety shower ref. PRESTO brand 85755 with manual control by rigid rod with balancing counterweight. Body in treated brass with red epoxy finish. Model with 1 fixed female head G3 / 4 '', shut-off valve, supply on visible piping. Complies with ANSI Z 358.1 and EN 15154.1-2 standards.