86203 - WALL-MOUNTED ABOVE DOOR EMERGENCY BODY SHOWER
Safety shower ref. PRESTO brand 86203 with manual control by rigid rod with balancing counterweight. Body in treated brass with red epoxy finish. Model with 1 fixed female head G 3/4 '', shut-off valve, supply on visible piping. To be placed above a door, to the left or to the right of the door. Complies with ANSI Z 358 1 and EN 15154.1-2 standards.