IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "RevitIdentifiers [VersionGUID: 9afec3e4-8e82-4a76-aeae-fbf6823c1ee5, NumberOfSaves: 0]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
File name: "14260 - presto.ifc"
Time stamp: "2025-06-04T22:31:34"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.80.32 - IFC 22.7.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "mostafa.etmanHDZVT" of Organization (no name given)
  Owner history of Person "mostafa.etmanHDZVT" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1749061893 (2025-06-04T18:31:33Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "14260:14260 - PRESTO" | object type "14260:14260 - PRESTO" | names: "14260:14260 - PRESTO:351430" | material: materials ("Wall Texture, Orange Peel", "Bronze", "Bronze, Architectural", "Stainless Steel, Polished") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Constraints, Phasing, Mechanical, Dimensions
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:8mm Head" | elevation 4000.0000000000005

Types
  IFCDISTRIBUTIONELEMENTTYPE "14260:14260 - PRESTO" | 1 occurrence | material: materials ("Wall Texture, Orange Peel", "Bronze", "Bronze, Architectural", "Stainless Steel, Polished") | property sets: Electrical - Loads, Constraints, Mechanical, Identity Data, Other, Pset_ManufacturerTypeInformation

Property sets
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "14260:14260 - PRESTO" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "14260:14260 - PRESTO" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 4000.0000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 3204.6217462812519 (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule Level = "Level 1" (IFCLABEL)
    Work Plane = "<not associated>" (IFCTEXT)
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.073108653257044215 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00039779435682274776 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 2" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "1" (IFCTEXT)
    Materials & Finish = "Crude brass body and stop valve / - Remote control push button made in Brass chrome plated" (IFCTEXT)
    Range = "Flush valve for toilet with remote control" (IFCTEXT)
    Ref = "14260 - PRESTO 1000 XL TC Induct mounting" (IFCTEXT)
    Security = "Anti-siphonic device / - Patented anti-blocking "S" system to avoid the water to flow continuously" (IFCTEXT)
    Volume of water delivered = "Adjustable from 6 to 9 / -Anti-water-hammering design /- Automatic 1 l/s flow limiter for a constant flow from 1.2 to 4 bar dynamic working pressure" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Description = "PRESTO 1000 XL TC Induct mounting" (IFCTEXT)
    Manufacturer = "PRESTO" (IFCTEXT)
    OmniClass Number = "23.45.00.00" (IFCTEXT)
    OmniClass Title = "Sanitary, Laundry, and Cleaning Equipment" (IFCTEXT)
    Type Name = "14260 - PRESTO" (IFCTEXT)
    URL = "https://www.prestodatashare.com/espacedoc/Fiches_Techniques/GB/14260.pdf" (IFCTEXT)
    brand = "LES ROBINETS PRESTO" (IFCTEXT)
    ref = "14260 - PRESTO 1000 XL TC Induct mounting" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "8mm Head" (IFCLABEL)
    Type Id = "305" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "14260" (IFCLABEL)
    Family and Type = "14260: 14260 - PRESTO" (IFCLABEL)
    Type = "14260 - PRESTO" (IFCLABEL)
    Type Id = "351401" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "14260" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    System Classification = "Hydronic Return,Hydronic Supply" (IFCTEXT)
  Mechanical | properties | on 1 type object
    - Hydraulic supply = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    -Delivered with = "1 Ball valve / - 1 Remote control for induct mounting 15 to 200mm with clamping nuts / - 1 PVC angled pipe / - 1 Nozzle / - 1 Instruction manual" (IFCTEXT)
    > Standards & approvals = "Acoustic class II / - Brass body in accordance with EN 1982, EN 12164, EN 12165 / - Molded chrome-plated body in accordance with EN 12540 / - 200-hour neutral salt spray resistant (NSS) in accordance with ISO 9227" (IFCTEXT)
    Recommended pressure = 3. (IFCPRESSUREMEASURE) [PASCAL]
    flow = 6. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    flow time = 1. (IFCTIMEMEASURE) [SECOND]
    min flow = 1. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    pressure = 4.9999999999999991 (IFCPRESSUREMEASURE) [PASCAL]
  Constraints(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    power = 0. (IFCPOWERMEASURE) [WATT]
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "PRESTO" (IFCLABEL)