IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "RevitIdentifiers [VersionGUID: 9a254563-b924-4ad8-896a-2db07c721058, NumberOfSaves: 0]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
File name: "38022-presto.ifc"
Time stamp: "2025-05-30T23:14:47"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.80.32 - IFC 22.7.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "mostafa.etmanHDZVT" of Organization (no name given)
  Owner history of Person "mostafa.etmanHDZVT" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1748632487 (2025-05-30T19:14:47Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "38022-presto:38022- Les Robinets PRESTO" | object type "38022-presto:38022- Les Robinets PRESTO" | names: "38022-presto:38022- Les Robinets PRESTO:391669" | material: materials ("Default New Material", "Chromed brass.") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Constraints, Phasing, Mechanical, Materials and Finishes
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:8mm Head" | elevation 4000.0000000000005

Types
  IFCDISTRIBUTIONELEMENTTYPE "38022-presto:38022- Les Robinets PRESTO" | 1 occurrence | material: materials ("Default New Material", "Chromed brass.") | property sets: Constraints, Mechanical, Materials and Finishes, Identity Data, Other

Property sets
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "38022- Les Robinets PRESTO" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "38022- Les Robinets PRESTO" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 4000.0000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 4035.384234561453 (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule Level = "Level 1" (IFCLABEL)
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.012855409096350728 (IFCAREAMEASURE) [SQUARE_METRE]
    HEIGHT = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00013585410710061731 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 2" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Delivered with = "Flat gasket 1 Filter gasket 2 Union nuts 3/4" (20x27) for 14x16 mm tube Instruction manual" (IFCTEXT)
    Mark = "24" (IFCTEXT)
    Range = "Timed flow single tap for shower" (IFCTEXT)
    Ref = "38022 - PRESTO P 50 single tap" (IFCTEXT)
    Standards & approvals = "Lead-free brass in accordance with NF EN1982, EN12164, NF EN 12165, 4MS, RoHS, Reach, NSF-372, UBA list compliant. / -Dezincification compliant with ISO 6509 and NDZ. / -200-hour neutral salt spray resistant (NSS) in accordance with NF ISO 9227." (IFCTEXT)
  Identity Data | properties | on 1 type object
    Description = "Flat gasket 1 Filter gasket 2 Union nuts 3/4" (20x27) for 14x16 mm tube Instruction manual" (IFCTEXT)
    Model = "38022" (IFCTEXT)
    OmniClass Number = "23.45.00.00" (IFCTEXT)
    OmniClass Title = "Sanitary, Laundry, and Cleaning Equipment" (IFCTEXT)
    Type Name = "38022- Les Robinets PRESTO" (IFCTEXT)
    URL = "https://www.prestodatashare.com/espacedoc/Fiches_Techniques/GB/38022.pdf" (IFCTEXT)
    brand = "Les Robinets PRESTO" (IFCTEXT)
    range = "Timed flow single tap for shower" (IFCTEXT)
    ref = "38022 - PRESTO P 50 single tap" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "8mm Head" (IFCLABEL)
    Type Id = "305" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "38022-presto" (IFCLABEL)
    Family and Type = "38022-presto: 38022- Les Robinets PRESTO" (IFCLABEL)
    Type = "38022- Les Robinets PRESTO" (IFCLABEL)
    Type Id = "391631" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "38022-presto" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    System Classification = "Hydronic Supply" (IFCTEXT)
  Mechanical | properties | on 1 type object
    - Hydraulic supply = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Recommended pressure = 299999.99999999994 (IFCPRESSUREMEASURE) [PASCAL]
    flow = 0.10000000000000001 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    flow time = 30. (IFCTIMEMEASURE) [SECOND]
    min pressure = 99999.999999999985 (IFCPRESSUREMEASURE) [PASCAL]
    pressure = 499999.99999999994 (IFCPRESSUREMEASURE) [PASCAL]
  Materials and Finishes | properties | on 1 object (1 IFCFLOWTERMINAL)
    Material = "Default New Material" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    material1 = "Chromed brass." (IFCLABEL)
  Constraints(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)